Sensors Rate # Make Location Height 3-Dimensional sonic anemometer

10 Hz 2 Applied Technologies model K

50m flux twr 10m, (5m)

250m flux twr 10m, (5m) 3-Dimensional sonic anemometer

20 Hz 2 Univ of Washington 100m flux twr 10m, (5m)

175m flux twr 10m, (5m) Fast-response temperature 20 Hz 4 Atmos. Instrum. Res. 50m flux twr 10m, (5m) 100m flux twr 10m, (5m) 175m flux twr 10m, (5m) 250m flux twr 10m, (5m) Fast-response humidity 20 Hz 2 Campbell Scientific Kr hygrometer

50m flux twr 10m, (5m)

250m flux twr 10m, (5m) Fast SF6 sensor 3 Hz 4 Scientech 50m flux twr 10m, (5m) 100m flux twr 10m, (5m) 175m flux twr 10m, (5m) 250m flux twr 10m, (5m) Wind speed and direction 1 Hz 5 NCAR propvane 50m prop twr 1.5m, 3m, 5m, 7.5m, 10m Platinum resistance thermometer and humitter

1 Hz 5 NCAR psychrometer 250m psyc twr 1.5m, 3m, 5m, 7.5m, 10m Pressure sensor 1 Hz 3 NCAR barometer 250m psyc twr 0.3m Pyranometer 1 Hz 2 Eppley Radiation stand 3m Pyrgeometer 1 Hz 2 Eppley Radiation stand 3m Net radiometer 1 Hz 1 Micromet Systems Q5 Radiation stand 3m Surface infrared radiometer 1 Hz 1 Everest Interscience Radiation stand 3m Soil temperature 1 Hz 12 NCAR multiplexer Bush 1, 3, 5, 7cm deep Grass 1, 3, 5, 7cm deep Sand 1, 3, 5, 7cm deep Soil heat flux 1 Hz 3 Micromet Systems Bush 8cm deep Grass 8cm deep Sand 8cm deep